{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["List1","List2","List3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"List1","index":0,"n_rows":41,"n_cols":31,"rows_kept":41,"cut":false,"hidden":false,"merged":[[22,19,22,23],[21,27,21,28],[22,27,22,28],[49,19,52,25],[13,19,13,25],[15,19,15,25],[16,19,16,25],[26,19,26,23],[27,19,27,23],[30,19,30,22],[14,19,14,22],[36,19,36,22],[37,19,37,22],[38,19,38,22],[18,19,18,23],[19,19,19,23],[20,19,20,23],[17,19,17,23],[21,19,21,23],[8,22,8,28],[10,19,10,22],[23,19,23,23],[24,19,24,23],[25,19,25,23],[11,19,11,25],[12,19,12,25],[11,27,11,28],[12,27,12,28],[13,27,13,28],[15,27,15,28],[18,27,18,28],[19,27,19,28],[20,27,20,28],[16,27,16,28],[17,27,17,28],[39,19,39,22],[40,19,40,22],[28,19,29,30],[33,19,33,22],[34,19,34,22],[31,19,32,30]]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"VÝKAZ VÝMĚR"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NÁZEV",null,null,null,null,null,null,"m.j.",null,"množství","cena/m.j.","cena celkem"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"demontáž eternitu",null,null,null,null,null,null,"m2",177.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ekologická likvidace eternitu",null,null,null,null,null,null,"t",1.98]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"demontáž nároží,hřebene",null,null,null,null,null,null,"m",29]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"pronájem kontejneru,odvoz eternitu",null,null,null,null,null,null,"kpl ",null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"odvětrávací hlavice ",null,null,null,null,null,null,"ks",16]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"střešní výlez",null,null,null,null,null,null,"ks",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"komínová lávka",null,null,null,null,null,null,"ks",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"sněhová zábrana",null,null,null,null,null,null,"ks",125]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ventilační prostup",null,null,null,null,null,null,"ks",2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodávka a montáž podstřešní hydroizolace",null,null,null,null,null,null,"m2",215]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodávka krytiny dle alternativy 1) nebo 2)",null,null,null,null,null,null,"m2",177.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montáž krytiny dle alter.1) nebo 2)",null,null,null,null,null,null,"m2",177.4]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodávka a montáž nároží a hřebene",null,null,null,null,null,null,"m",null,29]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"založení krytiny",null,null,null,null,null,null,"m",null,55.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"přiřezání krytiny",null,null,null,null,null,null,"m",null,135.80000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"přesun hmot",null,null,null,null,null,null,"t",null,2.58]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"spojovací prostředky ",null,null,null,null,null,null,"m2",null,177.4]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"lešení,montáž,demontáž,májem",null,null,null,null,null,null,"m2",null,250]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"demontáž klemp.prvků,žlabů a svodů",null,null,null,null,null,null,"kpl",null,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"oplechování okapů vč.nátěrů",null,null,null,null,null,null,"m",null,55.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodávka a montáž žlabů a svodů vč.nát.",null,null,null,null,null,null,"m",null,55.7]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"závětrná lišta rš.330 mm vč.nátěru",null,null,null,null,null,null,"m",null,34.299999999999997]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"oplechování zdí rš.330 mm vč.nátěrů",null,null,null,null,null,null,"m",null,26]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"oplechování úžlabí rš.500 mm vč.nát.",null,null,null,null,null,null,"m",null,14.25]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"montáž svodů pr.100 mm",null,null,null,null,null,null,"m",null,24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"dodání a montáž kotlíků 100/330 mm vč.nát.",null,null,null,null,null,null,"ks",null,5]

{"sheet":"List2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"List3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}