Opis predmetov zákazky

1.

* SIMICAN FD - Rest-bus simulátor dvoch zberníc CAN FD a dvoch zberníc LIN s káblom s OBD konektorom

- Zariadenie schopné simulovať celú elektroniku vozidla koncernu Volkswagen pre potreby prípadného pripojenia ľubovoľných elektronických komponentov a ich následnej diagnostiky a zálohovania dát za účelom individuálnej identifikácie.

- Simulácia zberníc platformy MQB, MQB2020, MEB

 - počet zariadení ....................................................................................................... 3 ks

2.

* Prístrojová doska Škoda obj. č. 654 920 790 A (Škoda Scala) .................................. 1 ks
* Prístrojová doska Škoda obj. č. 565 920 751 (Škoda Kodiaq) ................................... 1 ks
* Anténna cievka obj. č. 5K0 953 254 A (k prístrojovej doske obj. č. 565 920 751) ... 1 ks
* Anténna cievka obj. č. 2Q0 953 254 (k prístrojovej doske obj. č. 654 920 790 A) ... 1 ks

3.

* čítačka transpondérov kľúčov (TANGO), ktorá podporuje transpondéry:

**- Philips transponders:**

PCF7930-31 writing, reading

PCF7935 writing, reading, shadow memory, crypto calculator

PCF7936 writing, reading, modes password, crypto, Manchester & Biphase encodings

PCF7941 transponder, remote, eeprom, Manchester & Biphase encodings

PCF7942 transponder, remote, eeprom, Manchester & Biphase encodings

PCF7943 transponder, remote, Manchester & Biphase encodings

PCF7944 transponder, remote, eeprom, Manchester & Biphase encodings

PCF7945 transponder, remote, eeprom, Manchester & Biphase encodings

PCF7946 transponder, remote, Manchester & Biphase encodings

PCF7947 transponder, remote, eeprom, Manchester & Biphase encodings

PCF7952 transponder, remote, eeprom, Manchester & Biphase encodings

PCF7961 transponder, remote, Manchester & Biphase encodings

\*Auto switching between PCF7936 PCF7961 windows if invalid type detected.

\*Autodetect manchester / biphase

**- Temic transponders:**

Temic 11 reading , writing to T5

Temic 12 reading , writing to T5

Temic 8C reading

**- Megamos transponders:**

Megamos (13) reading , writing to T5 , emulating on PCF7930-35

Megamos (48) reading, writing, PIN, unlock by PIN,

full range of memory contents, crypto calculation

Megamos CRYPTO-2 (8E) read ID, read/write EEPROM, write Cryptokey

**- Texas transponders:**

Tiris (4C) reading

Tiris (4D) DST crypto reading, writing, crypto calculator

Tiris (4E) DST crypto reading, writing, crypto calculator

Tiris (8C) reading

**- Atmel:**

TK5551M (T5 replacement)

- počet zariadení .................................................................................................... 3 ks

4.

* Konektor CANON 9 – zásuvka na kábel (napr. D-SUB konektor CAN 9 Z) ........ 15 ks
* Konektor CANON 9 – vidlica na kábel (napr. D-SUB konektor CAN 9 V) ...........15 ks
* Kryt na konektor CANON 9 vrátane skrutiek ........................................................ 30 ks

# Predlžovací sériový kábel CANON 9 – vidlica - zásuvka, 2m ................................ 9 ks

* Pár konektorov 3 piny s vodičmi (napr. pár superseal konektorov, 3 piny) ........... 15 ks
* Pár konektorov 6 pinov s vodičmi (napr. pár superseal konektorov, 6 pinov) ....... 15 ks
* Plochý viacžilový kábel 8x0,5mm2

(napr. plochý viacžilový kábel farebný VFL 8x0,50) ............................................ 20m

Termín dodania: do 31. 07. 2021